SdFat

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Sd2Card Member List

This is the complete list of members for Sd2Card, including all inherited members.

begin(uint8_t csPin=SS, SPISettings settings=SD_SCK_MHZ(50)) | Sd2Card | inline
SdSpiCard::begin(SdSpiDriver *spi, uint8_t csPin, SPISettings spiSettings) | SdSpiCard |
cardSize() | SdSpiCard |
erase(uint32_t firstBlock, uint32_t lastBlock) | SdSpiCard |
eraseSingleBlockEnable() | SdSpiCard |
error(uint8_t code) | SdSpiCard | inline
errorCode() const | SdSpiCard | inline
errorData() const | SdSpiCard | inline
isBusy() | SdSpiCard |
readBlock(uint32_t lba, uint8_t *dst) | SdSpiCard |
readBlocks(uint32_t lba, uint8_t *dst, size_t nb) | SdSpiCard |
readCID(cid_t *cid) | SdSpiCard | inline
readCSD(csd_t *csd) | SdSpiCard | inline
readData(uint8_t *dst) | SdSpiCard |
readOCR(uint32_t *ocr) | SdSpiCard |
readStart(uint32_t blockNumber) | SdSpiCard |
readStatus(uint8_t *status) | SdSpiCard |
readStop() | SdSpiCard |
SdSpiCard() | SdSpiCard | inline
spiStart() | SdSpiCard |
spiStop() | SdSpiCard |
syncBlocks() | SdSpiCard | inline
type() const | SdSpiCard | inline
writeBlock(uint32_t lba, const uint8_t *src) | SdSpiCard |
writeBlocks(uint32_t lba, const uint8_t *src, size_t nb) | SdSpiCard |
writeData(const uint8_t *src) | SdSpiCard |
writeStart(uint32_t blockNumber) | SdSpiCard |
writeStart(uint32_t blockNumber, uint32_t eraseCount) | SdSpiCard |
writeStop() | SdSpiCard |